**Internal grille LGR 82/6**

Internal grille with front frame.

For installation in folded spiral-seams ducts.

With horizontal, rotatable air operated lamella with fitted bearings, located on the front side.

Air flow control by means of adjustable slot slides.

Ideally (DN 250 for 65 mm mounting height, DN 500 for 115 mm mounting height), the internal grille is fully on the duct.

With visible screw holes.

Technical data

|  |  |
| --- | --- |
| Article: | LGR 82/6 |
| Air direction: | Ventilation and air extraction |
| Practical air throughput at 75% opening of the slot slide: | 300 m³/h - 500 m³/h |
| Installation: | Inside |
| Installation site: | Duct |
| Material: | Sheet steel, galvanised |
| Weight: | 1,49 kg |
| Weight including packaging: | 1,73 kg |
| Suitable for nominal size: | 140 mm - 400 mm (ideal 250 mm) |
| Width: | 858 mm |
| Height: | 113 mm |
| Depth: | 56 mm |
| Width with packaging: | 890 mm |
| Height with packaging: | 120 mm |
| Depth with packaging: | 70 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513582 |
| Article number: | 0151.0358 |

Manufacturer: MAICO

LGR 82/6 Internal grille