**Shell kit PP 60 KA-SRL**

Shell kit for fitting in the external wall.

Scope of delivery:

Extra long PVC wall sleeve (700 mm) with two plaster protective covers and eight shims for aligning sleeve in wall hole.

External cover made of stainless steel.

Is needed as an accessory for the PP 60 K-SE final assembly kit.

Technical data

|  |  |
| --- | --- |
| Article: | PP 60 KA-SRL |
| Air flow volume: | 17 m³/h / 22 m³/h / 30 m³/h / 41 m³/h / 50 m³/h |
| Installation site: | Outside wall |
| Installation position: | horizontal |
| Material: | Stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 2,582 kg |
| Weight including packaging: | 3,508 kg |
| Nominal size: | 200 mm |
| Width: | 745 mm |
| Height: | 286 mm |
| Depth: | 250 mm |
| Width with packaging: | 715 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 275 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799952169 |
| Article number: | 0095.0216 |

Manufacturer: MAICO

PP 60 KA-SRL Shell kit