**External cover PPB 30 AE**

External cover made from brushed stainless steel (V4A).

The integrated air-redirection keeps the exhaust air away from the outside wall. This greatly minimises discolouration and dirt deposits on the external façade.

Is recommended when the units are used in areas exposed to the wind.

An external cover is needed as an accessory for the PPB 30 K and PPB 30 O final assembly kits.

Technical data

|  |  |
| --- | --- |
| Article: | PPB 30 AE |
| Installation site: | Outside wall |
| Installation position: | horizontal |
| Housing material: | Stainless steel, brushed |
| Colour: | Stainless steel, brushed |
| Weight: | 1,6 kg |
| Weight including packaging: | 1,8 kg |
| Width: | 253 mm |
| Height: | 258 mm |
| Depth: | 67 mm |
| Width with packaging: | 295 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 86 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991762 |
| Article number: | 0093.1499 |

Manufacturer: MAICO

PPB 30 AE External cover