**Surface-mounted housing ER GH AP**

Model without fire protection

Surface-mounted housing with DN 75/80 plastic exhaust socket with airstream-operated plastic backflow preventer.

Airstream-operated plastic backflow preventer with simultaneous function as a cold smoke barrier.

Special features

For applications in accordance with DIN 18017-3.

Features

Surface-mounted housing to accommodate the ER EC fan insert in combination with the covers of the ER-A... series.

Installation in bathrooms, WCs and open-plan kitchens.

Wall or ceiling installation possible.

Housing can be rotated, so the exhaust socket can be connected to the main duct at the top left or top right.

Electrical connection at rear.

Simple electrical wiring on practical pin connector terminal.

DN 75/80 connection diameter.

Plastic parts, normally inflammable, according to DIN 4102-1 class B 2 (according to EN 13501-1).

Colour: traffic white, similar to RAL 9016.

Easy installation.

Technical data

|  |  |
| --- | --- |
| Article: | ER GH AP |
| Model: | without fire protection |
| Air direction: | Air extraction |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Degree of protection: | IP X5 |
| Mains cable: | 3/5 x 1.5 mm² |
| Installation site: | Wall / ceiling |
| Type of installation: | Surface-mounted |
| Housing material: | ABS plastic |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,62 kg |
| Weight including packaging: | 0,85 kg |
| Fire protection: | No |
| Air outlet direction: | at rear |
| Connection diameter: | 75 mm / 80 mm |
| Width: | 276 mm |
| Height: | 276 mm |
| Depth: | 180 mm |
| Width with packaging: | 350 mm |
| Height with packaging: | 140 mm |
| Depth with packaging: | 290 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799843528 |
| Article number: | 0084.0352 |

Manufacturer: MAICO

ER GH AP Surface-mounted housing