**Room air control RLS T2 WS**

Features

Modern intelligent touch screen control panel with graphic colour IPS display.

Display size 800 x 400 pixels.

Display diagonal 4.3.

With 16 MB of memory.

With NTC room temperature sensor (-20°C to +50°C).

With mini USB port.

With 4-wire bus connection (RS 485 incl. power supply).

Micro SD card slot.

Up to 5 ventilation units can be controlled with 1 RLS TS WS.

Technical data

|  |  |
| --- | --- |
| Article: | RLS T2 WS |
| Type of voltage: | DC voltage |
| Rated voltage: | 12 V DC |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Plastic/glass |
| Synthetic material definition: | PVC-free polystyrene |
| Colour: | white |
| Weight: | 0,21 kg |
| Weight including packaging: | 0,3 kg |
| Width: | 127 mm |
| Height: | 93 mm |
| Depth: | 50 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 51 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992660 |
| Article number: | 0157.1656 |

Manufacturer: MAICO

RLS T2 WS Room air control