**Sound-absorbing element PP 45 SE**

Sound-absorbing element as optional accessory for PP 45 O, PP 45 K and PP 45 RC final assembly kit.

Is used to reduce the sound power level and increase the sound insulation level.

Reduction in sound power level of up to 2 dB(A) with one sound-absorbing element.

Reduction in sound power level of up to 5 dB(A) with two sound-absorbing elements (turned 45°).

Scope of delivery:

1 x outer ring

1 x inner part

The inner part only serves as transport protection and has to be removed before installation in the final assembly kit.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 SE |
| Installation site: | Wall |
| Material: | melamine resin |
| Colour: | grey |
| Weight: | 0,02 kg |
| Weight including packaging: | 0,02 kg |
| Fire protection: | Fire-proof class B1 |
| External diameter: | 154 mm |
| Width: | 154 mm |
| Height: | 154 mm |
| Depth: | 100 mm |
| Width with packaging: | 156 mm |
| Height with packaging: | 156 mm |
| Depth with packaging: | 101 mm |
| Total insertion loss: | 2 dB |
| Insertion loss note: | with 2x PP45 SE (turned 45°): 2.5-5 dB(A) |
| Sound insulation: | yes |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799933083 |
| Article number: | 0093.0308 |

Manufacturer: MAICO

PP 45 SE Sound-absorbing element