**Wall-mounted fan EMA 17**

Technical data

|  |  |
| --- | --- |
| Article: | EMA 17 |
| Air flow volume: | 260 m³/h |
| Rotating speed: | 2.800 1/min |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Power consumption: | 68 W |
| Imax: | 0,32 A |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 2,85 |
| Pulley integrated: | - |
| Packing unit: | 1 piece |
| Article number: | 080279 |

Manufacturer: MAICO

EMA 17 Wall-mounted fan