**Shell kit PP 60 KA-SR**

Features

Shell kit for fitting in the external wall.

Scope of delivery:

PVC wall sleeve with two plaster protective covers and eight shims for aligning sleeve in wall hole.

External cover made of stainless steel.

Is needed as accessory for PP 60 K-SE final assembly set.

Technical data

|  |  |
| --- | --- |
| Article: | PP 60 KA-SR |
| Air flow volume: | 17 m³/h / 22 m³/h / 30 m³/h / 41 m³/h / 50 m³/h |
| Installation site: | Outside wall |
| Installation position: | horizontal |
| Material: | Stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 2,2 kg |
| Weight including packaging: | 2,988 kg |
| Nominal size: | 200 mm |
| Width: | 286 mm |
| Height: | 250 mm |
| Depth: | 503 mm |
| Width with packaging: | 270 mm |
| Height with packaging: | 275 mm |
| Depth with packaging: | 615 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799952053 |
| Article number: | 0095.0205 |

Manufacturer: MAICO

PP 60 KA-SR Shell kit