**Air filter, replacement RF 35**

Replacement filter for TFE... air filter.

Technical data

|  |  |
| --- | --- |
| Article: | RF 35 |
| Installation position: | vertical / horizontal |
| Weight: | 0,42 kg |
| Weight including packaging: | 1,03 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Suitable for nominal size: | 355 mm |
| Width: | 458 mm |
| Height: | 445 mm |
| Depth: | 6 mm |
| Width: | 395 mm |
| Height: | 395 mm |
| Width with packaging: | 485 mm |
| Height with packaging: | 485 mm |
| Depth with packaging: | 65 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799936916 |
| Article number: | 0093.0691 |

Manufacturer: MAICO

RF 35 Air filter, replacement