**Second room extraction system ER-ZR**

Second room connection kit with mounting couplings, internal grille and filter.

In accordance with DIN 18017-3, can be combined with the following types: ER 100, ER 100 VZ, ER 100 VZ 15, ER 100 VZC, ER 100 G, ER 100 I, ER 100 D und ER EC with ER-AK/ER-AH/ER-AB covers.

Accessories: ZRF replacement air filter.

Technical data

|  |  |
| --- | --- |
| Article: | ER-ZR |
| Air direction: | Air extraction |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,18 kg |
| Weight including packaging: | 0,26 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 100 mm |
| Width with packaging: | 155 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 120 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799990314 |
| Article number: | 0093.1025 |

Manufacturer: MAICO

ER-ZR Second room extraction system