**Disk valve, metal TM 10**

Disk valves for air extraction.

Linear air flow control via rotatable valve disk.

Assembly using installation frames.

Mounting frames and fan housings are linked using a bayonet closure.

Recommended accessories: FFE grease filter element for use in rooms where the exhaust air contains grease (e.g. kitchens etc.).

Technical data

|  |  |
| --- | --- |
| Article: | TM 10 |
| Air direction: | Air extraction |
| Max. volumetric flow: | 30 m³/h |
| Material: | Sheet steel, stove-enamelled |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,41 kg |
| Weight including packaging: | 0,41 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 134 mm |
| Height: | 134 mm |
| Depth: | 83 mm |
| Width with packaging: | 140 mm |
| Height with packaging: | 140 mm |
| Depth with packaging: | 120 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799511946 |
| Article number: | 0151.0194 |

Manufacturer: MAICO

TM 10 Disk valve, metal