**Flexible steel duct SFR 80**

Flexible single-grooved folded spiral-seams duct made of galvanised sheet steel to be used as connection to the main duct, in accordance with DIN 18017-3.

Non-combustible in accordance with DIN 4102 class A1 (building material classification).

Length details: extended length.

Technical data

|  |  |
| --- | --- |
| Article: | SFR 80 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 0,46 kg |
| Weight including packaging: | 0,65 kg |
| Suitable for nominal size: | 80 mm |
| Length: | 1,2 m |
| Width: | 1.200 mm |
| Height: | 90 mm |
| Depth: | 90 mm |
| Width with packaging: | 620 mm |
| Height with packaging: | 100 mm |
| Depth with packaging: | 100 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799550723 |
| Article number: | 0055.0072 |

Manufacturer: MAICO

SFR 80 Flexible steel duct