**AK 16**

Shutter for air extraction.

Technical data

|  |  |
| --- | --- |
| Article: | AK 16 |
| Air direction: | Air extraction |
| Loss of pressure: | 10 Pa |
| Installation: | outside |
| Type of installation: | Surface-mounted |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Pearl white, similar to RAL 1013 |
| Lamella colour: | Beige grey - similar to RAL 7006 |
| Weight: | 0,1 |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 160 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799510383 |
| Article number: | 0151.0038 |

Manufacturer: MAICO

AK 16