**Air quality controller EAQ 10/1**

Air quality controller for operating fans depending on the air quality.

With integrated air quality sensor for measuring the concentration of various gases and odours (e.g. carbon monoxide, methane, hydrogen, alcohol, tobacco smoke).

The sensitivity can be continuously set using a potentiometer.

Preset at factory.

With 2 LEDs to display the operating state and the air quality.

Ready after approx. 5 min.

Reaction time: < 1 min.

Overrun time: 1 to 3 minutes (depending on the degree of pollution).

Safety instructions

EAQ 10/1 should not be used in security applications.

Technical data

|  |  |
| --- | --- |
| Article: | EAQ 10/1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load: | 10 A |
| Degree of protection: | IP 30 |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,24 kg |
| Weight including packaging: | 0,32 kg |
| Width: | 126 mm |
| Height: | 74 mm |
| Depth: | 24 mm |
| Width with packaging: | 190 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577775 |
| Article number: | 0157.0777 |

Manufacturer: MAICO

EAQ 10/1 Air quality controller