**EnOcean extension module PP 45 EO**

To convert the electric signals to EnOcean radio.

So that the PP 45 RC and PPB 30 RC units can be controlled.

Is connected to the RLS 45 K room air control using the RS485 interface.

A system combination of wired PP 45 K units and PP 45 RC / PPB 30 RC radio devices is thereby possible.

The PP 45 EO extension module can be used to integrate further EnOcean modules, e.g. radio sensors (H, CO2).

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 EO |
| Installation site: | Wall |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,17 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 49 mm |
| Width with packaging: | 233 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799573623 |
| Article number: | 0157.0362 |

Manufacturer: MAICO

PP 45 EO EnOcean extension module