**Floor grille FFS-FGBW**

Hard-wearing standard floor grille, suitable for the FFS-BA floor outlet.

The floor grille made of white lacquered stainless steel has a modern design with a circular pattern of holes.

It is held in place with clamps that are positioned tight under the floor grille.

Scope of delivery

1 floor grille

1 sealing tape

Technical data

|  |  |
| --- | --- |
| Article: | FFS-FGBW |
| Model: | Design with circular pattern of holes |
| Type of installation: | Fastening with clamps |
| Material: | Stainless steel, painted white |
| Weight: | 0,31 kg |
| Weight including packaging: | 0,33 kg |
| Width: | 340 mm |
| Height: | 180 mm |
| Depth: | 3 mm |
| Width with packaging: | 311 mm |
| Height with packaging: | 240 mm |
| Depth with packaging: | 138 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799558910 |
| Article number: | 0055.0891 |

Manufacturer: MAICO

FFS-FGBW Floor grille