**Air filter, replacement ZF 35**

Replacement air filter for DTH 35 AIROTHERM air heater.

Technical data

|  |  |
| --- | --- |
| Article: | ZF 35 |
| Installation position: | vertical / horizontal |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,82 kg |
| Filter class: | ISO Coarse 45 % (G3) |
| Suitable for nominal size: | 350 mm |
| Width: | 645 mm |
| Height: | 400 mm |
| Depth: | 18 mm |
| Width with packaging: | 660 mm |
| Height with packaging: | 405 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 5 pieces |
| Suitable for products: | DTH 35 |
| Range: | C |
| GTIN (EAN): | 4012799932079 |
| Article number: | 0093.0207 |

Manufacturer: MAICO

ZF 35 Air filter, replacement