**Flexible flat duct FFS-R52**

Flexible plastic oval flat duct with internal duct.

Technical data

|  |  |
| --- | --- |
| Article: | FFS-R52 |
| Max. volumetric flow: | 45 m³/h |
| Volumetric flow: | 15 m³/h / 30 m³/h / 45 m³/h bei 0,3 Pa/m / 1,1 Pa/m / 2,5 Pa/m |
| Weight: | 13 kg |
| Weight including packaging: | 13 kg |
| Length: | 20 m |
| Width: | 132 mm |
| Height: | 52 mm |
| Depth: | 132 mm |
| Width with packaging: | 132 mm |
| Height with packaging: | 52 mm |
| Depth with packaging: | 132 mm |
| Packing unit: | 1 x 20 m roll |
| Range: | K |
| GTIN (EAN): | 4012799558705 |
| Article number: | 0055.0870 |

Manufacturer: MAICO

FFS-R52 Flexible flat duct