**Spacer ECA-AH**

Spacer for the connection of small room fans of the ECA 100 group. For ECA piano or ECA 100 ipro.. follow-up models, the spacer has to be adjusted by the customer.

Through the use of the ECA-AH, the small room fan can be built into flat channel elbows without projection.

Do not install on windows or laminated glass.

Scope of delivery: Spacer with 4 spacing elements, 2 80 mm wood screws.

Technical data

|  |  |
| --- | --- |
| Article: | ECA-AH |
| Installation site: | Wall / Ceiling |
| Material: | Synthetic material |
| Colour: | White |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,294 kg |
| Width: | 151 mm |
| Height: | 151 mm |
| Depth: | 56 mm |
| Width with packaging: | 158 mm |
| Height with packaging: | 158 mm |
| Depth with packaging: | 120 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799924869 |
| Article number: | 0092.0486 |

Manufacturer: MAICO

ECA-AH Spacer