**Cleaning kit MF-R90**

Cleaning kit for cleaning MF-F flexible steel ducts.

A cleaning ball is placed in the ventilation duct in the MF-V... air distributor and is then sucked to one of the air outlets using a vacuum cleaner. During this process, the cleaning ball removes residual dirt and dust from the flexible steel duct.

Packing unit: Vacuum cleaner adaptor and 2 cleaning balls.

Technical data

|  |  |
| --- | --- |
| Article: | MF-R90 |
| Weight: | 0,18 kg |
| Weight including packaging: | 0,2 kg |
| Suitable for nominal size: | 90 mm |
| Width: | 150 mm |
| Height: | 200 mm |
| Depth: | 90 mm |
| Width with packaging: | 152 mm |
| Height with packaging: | 202 mm |
| Depth with packaging: | 92 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799580133 |
| Article number: | 0058.0013 |

Manufacturer: MAICO

MF-R90 Cleaning kit