**Mounting foot FUI 71**

Mounting feet for the assembly of DAR/DAR Ex on walls, ceilings or brackets.

Protected against weathering by epoxy coating.

Technical data

|  |  |
| --- | --- |
| Article: | FUI 71 |
| Material: | Sheet steel, epoxy coated |
| Colour: | grey |
| Weight: | 3,1 kg |
| Weight including packaging: | 3,1 kg |
| Width: | 700 mm |
| Height: | 207 mm |
| Depth: | 40 mm |
| Width with packaging: | 700 mm |
| Height with packaging: | 207 mm |
| Depth with packaging: | 40 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799732266 |
| Article number: | 0073.0226 |

Manufacturer: MAICO

FUI 71 Mounting foot