**90° branch AB 125-125**

90° branches for folded spiral-seam ducts, incl. lip seal(s).

For connecting several air distributors to one supply or exhaust air duct.

Technical data

|  |  |
| --- | --- |
| Article: | AB 125-125 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 0,52 kg |
| Weight including packaging: | 0,52 kg |
| Width: | 250 mm |
| Height: | 182 mm |
| Depth: | 182 mm |
| Width with packaging: | 250 mm |
| Height with packaging: | 130 mm |
| Depth with packaging: | 182 mm |
| Nominal width of opening: | 125 mm |
| Nominal size branch: | 125 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553557 |
| Article number: | 0055.0355 |

Manufacturer:
MAICO

AB 125-125 90° branch