**Door contact switch TS 2**

Door contact switch as spare part for the WS 150 and WS 250 centralised ventilation units.

Designed as contact switch.

Technical data

|  |  |
| --- | --- |
| Article: | TS 2 |
| Type of voltage: | Alternating current |
| Rated voltage: | 125 V - 250 V |
| Weight: | 0,02 kg |
| Weight including packaging: | 0,06 kg |
| Width: | 30 mm |
| Height: | 40 mm |
| Depth: | 12 mm |
| Width with packaging: | 175 mm |
| Height with packaging: | 250 mm |
| Depth with packaging: | 20 mm |
| Packing unit: | 2 pieces |
| Range: | K |
| GTIN (EAN): | 4012799101505 |
| Article number: | E157.0887.0000 |

Manufacturer:

 MAICO

TS 2 Door contact switch