**Housing extension GVI 90**

For converting standard versions with short housing into a version with long housing.

Conversion possible directly on site.

Protects motor and impeller.

Protected against weathering by sheet steel with epoxy coating.

Special version:

Housing extensions for sizes 140 and 160 are available on request.

Technical data

|  |  |
| --- | --- |
| Article: | GVI 90 |
| Material: | Sheet steel, epoxy coated |
| Colour: | grey |
| Weight: | 30 kg |
| Weight including packaging: | 30 kg |
| Width: | 1.030 mm |
| Height: | 1.030 mm |
| Depth: | 340 mm |
| Width with packaging: | 1.030 mm |
| Height with packaging: | 1.030 mm |
| Depth with packaging: | 340 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799732037 |
| Article number: | 0073.0203 |

Manufacturer: MAICO

GVI 90 Housing extension