**Cover ABD ER 60/100 F**

Cover with filter and time strip as spare part for the ER 60 F and ER 100 F fan inserts.

It is possible to rotate the cover by ± 5°, to compensate for housings which have been fitted at an angle.

Technical data

|  |  |
| --- | --- |
| Article: | ABD ER 60/100 F |
| Housing material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,43 kg |
| Weight including packaging: | 0,67 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 250 mm |
| Height: | 250 mm |
| Depth: | 33 mm |
| Width with packaging: | 280 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 155 mm |
| Range: | B |
| GTIN (EAN): | 4012799101208 |
| Article number: | E059.1017.9101 |

Manufacturer: MAICO

ABD ER 60/100 F Cover