**Air filter, replacement ALDF 10 T**

ALDF 10: Replacement air filter for outside air opening ALD 10.

ALDF 10 T: Replacement air filter for outside air opening ALD 10 T.

Technical data

|  |  |
| --- | --- |
| Article: | ALDF 10 T |
| Installation position: | vertical / horizontal |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,01 kg |
| Type of filter: | Dust filter |
| Filter class: | ISO Coarse 30 % (G2) |
| Internal diameter: | 32 mm |
| External diameter: | 95 mm |
| Width: | 95 mm |
| Height: | 95 mm |
| Depth: | 65 mm |
| Width with packaging: | 160 mm |
| Height with packaging: | 190 mm |
| Depth with packaging: | 70 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 5 pieces |
| Suitable for products: | ALD 10 T |
| Range: | B |
| GTIN (EAN): | 4012799931553 |
| Article number: | 0093.0155 |

Manufacturer: MAICO

ALDF 10 T Air filter, replacement