**Shutter, pull device VD 60**

Airstream operated shutters with pull device for manual operation.

Can be used only in rooms up to 5 m high due to thermal convection.

For vertical air directions and air extraction only.

Technical data

|  |  |
| --- | --- |
| Article: | VD 60 |
| Air direction: | Air extraction |
| Material: | Sheet steel |
| Weight: | 9,6 kg |
| Weight including packaging: | 9,84 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 600 mm |
| Width with packaging: | 710 mm |
| Height with packaging: | 470 mm |
| Depth with packaging: | 710 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799931089 |
| Article number: | 0093.0108 |

Manufacturer: MAICO

VD 60 Shutter, pull device