**90° sheet metal elbow MF-B75**

90° short sheet metal elbow for holding the flexible MAICOFlex ventilation duct system. The MF-F flexible steel duct is slid into the elbow.

Each elbow is fitted with 2 push-in mounting brackets on each elbow end which enable rapid fixing of the flexible steel duct.

Aerodynamic shape.

Simple and rapid installation.

Technical data

|  |  |
| --- | --- |
| Article: | MF-B75 |
| Material: | Sheet steel, galvanised |
| Weight: | 0,28 kg |
| Weight including packaging: | 0,3 kg |
| Nominal size: | 75 mm |
| Width: | 164 mm |
| Height: | 80 mm |
| Depth: | 164 mm |
| Width with packaging: | 164 mm |
| Height with packaging: | 80 mm |
| Depth with packaging: | 164 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799180678 |
| Article number: | 0018.0067 |

Manufacturer: MAICO

MF-B75 90° sheet metal elbow