**Weather protection roof WSD 20-40**

Weather protection roof for EKR -2 exhaust air boxes.

The weather protection roof protects the motors of the exhaust air boxes and should be used if the EKR -2 boxes have no protection from the elements.

The WSD 20-40 weather protection roof fits all nominal sizes of the EKR -2 exhaust air box. It is simply fitted to the exhaust air box door with four tapping screws or rivets. Four holes made in the door in the factory show the exact position.

Technical data

|  |  |
| --- | --- |
| Article: | WSD 20-40 |
| Installation: | outside |
| Installation site: | Outside wall |
| Material: | Sheet steel, galvanised |
| Weight: | 1,5 kg |
| Weight including packaging: | 1,68 kg |
| Width: | 330 mm |
| Height: | 290 mm |
| Depth: | 130 mm |
| Width with packaging: | 335 mm |
| Height with packaging: | 305 mm |
| Depth with packaging: | 140 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490838 |
| Article number: | 0149.0083 |

Manufacturer: MAICO

WSD 20-40 Weather protection roof