**External cover PP 45 AK**

Plastic external cover.

Colour: traffic white, similar to RAL 9016.

With integrated condensation drip edge.

The grilles are flow-optimised to minimise air disturbances and the exhaust air is kept away from the exterior wall. This greatly minimises discolouration and dirt deposits on the external façade.

An external cover is needed as an accessory for the PP 45 K, PP 45 O and PP 45 RC final assembly kits.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 AK |
| Installation site: | Outside wall |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,3 kg |
| Weight including packaging: | 0,32 kg |
| Width: | 217 mm |
| Height: | 217 mm |
| Depth: | 42 mm |
| Width with packaging: | 225 mm |
| Height with packaging: | 225 mm |
| Depth with packaging: | 50 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799931768 |
| Article number: | 0093.0176 |

Manufacturer: MAICO

PP 45 AK External cover