**90° elbow, drawn B90-125**

90° elbow, drawn, incl. lip seals. For folded spiral-seam ducts.

E.g. for connecting WS 120 Trio, WS 160 Flat or WS 170 centralised ventilation units to folded spiral-seams ducts as alternative to SVR 125 plug connector.

Technical data

|  |  |
| --- | --- |
| Article: | B90-125 |
| Material: | Sheet steel |
| Weight: | 0,6 kg |
| Weight including packaging: | 0,6 kg |
| Nominal size: | 125 mm |
| Width: | 235 mm |
| Height: | 235 mm |
| Depth: | 235 mm |
| Width with packaging: | 235 mm |
| Height with packaging: | 235 mm |
| Depth with packaging: | 235 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553120 |
| Article number: | 0055.0312 |

Manufacturer: MAICO

B90-125 90° elbow, drawn