**Air filter, replacement KFF 9040-5**

Replacement air filter for sound-insulated flat box for supply air KFR/KFD, KFR -K/KFD -K and KFR -F/KFD -F.

Technical data

|  |  |
| --- | --- |
| Article: | KFF 9040-5 |
| Installation position: | vertical / horizontal |
| Weight: | 3,83 kg |
| Weight including packaging: | 3,92 kg |
| Type of filter: | Fine filters |
| Filter class: | ISO ePM1 55 % (F5) |
| Width: | 892 mm |
| Height: | 387 mm |
| Depth: | 96 mm |
| Width with packaging: | 893 mm |
| Height with packaging: | 388 mm |
| Depth with packaging: | 100 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799990611 |
| Article number: | 0093.1217 |

Manufacturer: MAICO

KFF 9040-5 Air filter, replacement