**Air filter, replacement Trio M5**

Replacement air filters for WS 120 Trio and Trio centralised ventilation units

Technical data

|  |  |
| --- | --- |
| Article: | Trio M5 |
| Installation position: | vertical / horizontal |
| Weight: | 0,08 kg |
| Weight including packaging: | 0,09 kg |
| Filter class: | ISO ePM10 ≥ 50 % (M5) |
| Width: | 205 mm |
| Height: | 167 mm |
| Depth: | 46 mm |
| Width with packaging: | 300 mm |
| Height with packaging: | 220 mm |
| Depth with packaging: | 53 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799991205 |
| Article number: | 0093.1452 |

Manufacturer: MAICO

Trio M5 Air filter, replacement