**Flexible coupling ELP 93**

Flexible couplings for mounting channel fans that are free from structure-borne noise.

With square flange connection frames made of galvanised steel.

Installation on the inlet and outlet sides.

Technical data

|  |  |
| --- | --- |
| Article: | ELP 93 |
| Installation site: | Channel |
| Material: | Synthetic material |
| Weight: | 3,3 kg |
| Weight including packaging: | 3,67 kg |
| Channel dimension: | 900 mm x 300 mm |
| Width: | 940 mm |
| Height: | 340 mm |
| Depth: | 150 mm |
| Width with packaging: | 970 mm |
| Height with packaging: | 360 mm |
| Depth with packaging: | 75 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799922636 |
| Article number: | 0092.0263 |

Manufacturer: MAICO

ELP 93 Flexible coupling