**TRE 0,4**

5-step transformers for setting speed.

To control AC fans.

With operating indicator light.

Additional switching contact (230 V) e.g. for controlling a shutter.

Technical data

|  |  |
| --- | --- |
| Article: | TRE 0,4 |
| Maximum load: | 0,4 A |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 1,05 |
| Weight including packaging: | 1,05 kg |
| Width: | 92 mm |
| Height: | 165 mm |
| Depth: | 77 mm |
| Width with packaging: | 110 mm |
| Height with packaging: | 90 mm |
| Depth with packaging: | 180 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799161103 |
| Article number: | 0016.0110 |

Manufacturer: MAICO

TRE 0,4