**Roof socket insulated, for flat roofs SOFI 50-56**

Flat roof socket for assembly of roof fans.

With non-flammable sound and heat insulation.

Technical data

|  |  |
| --- | --- |
| Article: | SOFI 50-56 |
| Material: | Sheet steel, galvanised |
| Housing material: | Sheet steel, galvanised |
| Colour: | Silver |
| Weight: | 18,7 kg |
| Weight including packaging: | 18,7 kg |
| Width: | 1.140 mm |
| Height: | 300 mm |
| Depth: | 1.140 mm |
| Width with packaging: | 1.140 mm |
| Height with packaging: | 300 mm |
| Depth with packaging: | 1.140 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799730507 |
| Article number: | 0073.0050 |

Manufacturer: MAICO

SOFI 50-56 Roof socket insulated, for flat roofs