**Air filter, replacement PF 100**

Replacement air filter for fresh air units.

Technical data

|  |  |
| --- | --- |
| Article: | PF 100 |
| Installation position: | vertical / horizontal |
| Weight: | 0,04 kg |
| Weight including packaging: | 0,34 kg |
| Type of filter: | Pollen filter |
| Filter class: | ISO ePM1 80 % (F7) |
| Width: | 225 mm |
| Height: | 95 mm |
| Depth: | 3 mm |
| Width: | 600 mm |
| Height: | 94 mm |
| Width with packaging: | 265 mm |
| Height with packaging: | 150 mm |
| Depth with packaging: | 150 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 5 pieces |
| Suitable for products: | POL 100, POL 100 Z |
| Range: | D |
| GTIN (EAN): | 4012799936510 |
| Article number: | 0093.0651 |

Manufacturer: MAICO

PF 100 Air filter, replacement