**Installation box EK 62/22**

Installation box for fitting in suspended ceilings.

For combination with LGA and LGZ internal grilles.

Technical data

|  |  |
| --- | --- |
| Article: | EK 62/22 |
| Installation: | Inside |
| Material: | Sheet steel, galvanised |
| Weight: | 5,64 kg |
| Weight including packaging: | 6,11 kg |
| Width: | 650 mm |
| Height: | 247 mm |
| Depth: | 333 mm |
| Width with packaging: | 665 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 350 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490869 |
| Article number: | 0149.0086 |

Manufacturer: MAICO

EK 62/22 Installation box