**90° branch AB 160-125**

90° branches for folded spiral-seam ducts, incl. lip seal(s).

For connecting several air distributors to one supply or exhaust air duct.

Technical data

|  |  |
| --- | --- |
| Article: | AB 160-125 |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 0,65 kg |
| Weight including packaging: | 0,65 kg |
| Width: | 250 mm |
| Height: | 220 mm |
| Depth: | 220 mm |
| Width with packaging: | 250 mm |
| Height with packaging: | 220 mm |
| Depth with packaging: | 220 mm |
| Nominal width of opening: | 125 mm |
| Nominal size branch: | 125 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553694 |
| Article number: | 0055.0369 |

Manufacturer: MAICO

AB 160-125 90° branch