**Power module PP 45 LT**

Power unit for extending the PushPull system to more than 6 units.

A further 6 units can be connected per power unit.

Is connected to the RLS 45 K or RLS 45 O room air control using the RS485 interface.

The commands of the RLS 45 K or RLS 45 O room air control are forwarded to the connected units by the PP 45 LT.

A maximum of three power units can be connected per room air control.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 LT |
| Rated voltage: | 230 V |
| Mains cable: | 2 x 1,5 mm² |
| Installation site: | Wall |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,11 kg |
| Weight including packaging: | 0,22 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 49 mm |
| Width with packaging: | 230 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799573616 |
| Article number: | 0157.0361 |

Manufacturer: MAICO

PP 45 LT Power module