**Intake socket ASI 45**

Intake socket for turbulence-reduced air intake.

Technical data

|  |  |
| --- | --- |
| Article: | ASI 45 |
| Air direction: | Ventilation and air extraction |
| Material: | Sheet steel, coated |
| Colour: | grey |
| Weight: | 1,1 kg |
| Weight including packaging: | 1,1 kg |
| Width: | 520 mm |
| Height: | 450 mm |
| Depth: | 55 mm |
| Width with packaging: | 520 mm |
| Height with packaging: | 450 mm |
| Depth with packaging: | 55 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799734406 |
| Article number: | 0073.0440 |

Manufacturer: MAICO

ASI 45 Intake socket