**Floor grille FFS-FG**

Hard-wearing designer floor grille, suitable for the FFS-BA floor outlet.

The floor grille made of brushed stainless steel has a modern long-slot design.

The mounting frame allows it to be lined up with the surrounding floor covering.

It is held in place with clamping pins.

Scope of delivery:

1 floor grille

1 holder

1 sealing tape

Technical data

|  |  |
| --- | --- |
| Article: | FFS-FG |
| Model: | Slot design |
| Type of installation: | with mounting frame, held in place with clamping pins |
| Material: | Stainless steel, brushed |
| Weight: | 0,95 kg |
| Weight including packaging: | 1,09 kg |
| Width: | 340 mm |
| Height: | 180 mm |
| Depth: | 30 mm |
| Width with packaging: | 350 mm |
| Height with packaging: | 205 mm |
| Depth with packaging: | 50 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799558897 |
| Article number: | 0055.0889 |

Manufacturer: MAICO

FFS-FG Floor grille