**Installation box EK 42/12**

Installation box for fitting in suspended ceilings.

For combination with LGA and LGZ internal grilles.

Technical data

|  |  |
| --- | --- |
| Article: | EK 42/12 |
| Installation: | Inside |
| Material: | Sheet steel, galvanised |
| Weight: | 2,79 kg |
| Weight including packaging: | 3,02 kg |
| Width: | 448 mm |
| Height: | 149 mm |
| Depth: | 244 mm |
| Width with packaging: | 470 mm |
| Height with packaging: | 220 mm |
| Depth with packaging: | 255 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490845 |
| Article number: | 0149.0084 |

Manufacturer: MAICO

EK 42/12 Installation box