**Wall sleeve WW90**

Accessories for mounting without shell installation kit for WS 75 decentralised ventilation unit.

Installation in the exterior wall with wall thicknesses up to 500 mm.

Technical data

|  |  |
| --- | --- |
| Article: | WW90 |
| Air flow volume: | 20 m³/h / 70 m³/h |
| Installation site: | Outside wall |
| Colour: | black (similar to RAL 9005 deep black) |
| Weight: | 0,45 kg |
| Weight including packaging: | 0,46 kg |
| Connection diameter: | 90 mm |
| Width: | 125 mm |
| Height: | 125 mm |
| Depth: | 500 mm |
| Width with packaging: | 270 mm |
| Height with packaging: | 135 mm |
| Depth with packaging: | 510 mm |
| Packing unit: | 1 set (2 pieces) |
| Range: | K |
| GTIN (EAN): | 4012799956648 |
| Article number: | 0095.0664 |

Manufacturer: MAICO

WW90 Wall sleeve