**Reducer, asymmetrical REDA55/220/55**

Features

Reduction asymmetrical, collar size. Surface: Sendzimir galvanised.

Technical data

|  |  |
| --- | --- |
| Article: | REDA55/220/55 |
| Housing material: | Sheet steel, Sendzimir galvanised |
| Weight including packaging: | 0 kg |
| Channel dimension: | 220 mm x Array x 55 mm |
| Reduction to channel dimension: | x/ x |
| Width with packaging: | 0 mm |
| Height with packaging: | 0 mm |
| Depth with packaging: | 0 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799557074 |
| Article number: | 0055.0707 |

Manufacturer: MAICO

REDA55/220/55 Reducer, asymmetrical