**Vertical flat duct elbow FFS-BV**

Plastic channel elbow 90°.

Vertical model.

With connection option for flexible flat duct.

Scope of delivery:

1 channel elbow

2 individual duct fixing adapters (FFS-RA)

Technical data

|  |  |
| --- | --- |
| Article: | FFS-BV |
| Volumetric flow: | 15 m³/h / 30 m³/h / 45 m³/h bei 1,1 Pa / 4,4 Pa, 10,0 Pa |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,21 kg |
| Width: | 207 mm |
| Height: | 98 mm |
| Depth: | 98 mm |
| Width with packaging: | 250 mm |
| Height with packaging: | 105 mm |
| Depth with packaging: | 160 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799558774 |
| Article number: | 0055.0877 |

Manufacturer: MAICO

FFS-BV Vertical flat duct elbow