**Air filter, replacement ZRF**

Replacement filter for ER-ZR second room connection kit and for AZE 100 and ESG 10/2 internal grilles.

Technical data

|  |  |
| --- | --- |
| Article: | ZRF |
| Installation position: | vertical / horizontal |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,02 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Suitable for nominal size: | 100 mm |
| Width: | 125 mm |
| Height: | 125 mm |
| Depth: | 10 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 45 mm |
| Packing unit: | 5 pieces |
| Range: | B |
| GTIN (EAN): | 4012799939238 |
| Article number: | 0093.0923 |

Manufacturer: MAICO

ZRF Air filter, replacement