**Cover – upper part ABDO ER-AB**

Cover for upper part as spare part for the ER-AB cover.

For model with motion detector with intelligent time module.

Technical data

|  |  |
| --- | --- |
| Article: | ABDO ER-AB |
| Housing material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,21 kg |
| Weight including packaging: | 0,38 kg |
| Width: | 280 mm |
| Height: | 33 mm |
| Depth: | 280 mm |
| Width with packaging: | 285 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 285 mm |
| Range: | B |
| GTIN (EAN): | 4012799100935 |
| Article number: | E059.2047.9000 |

Manufacturer: MAICO

ABDO ER-AB Cover – upper part