**Sealing DI WS 75**

Seal between ventilation unit and flush-mounted housing as spare part for the WS 75 Powerbox H semi-centralised ventilation units.

In this way, a mixture of supply and exhaust air volumetric flows is avoided.

Technical data

|  |  |
| --- | --- |
| Article: | DI WS 75 |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,16 kg |
| Width: | 224 mm |
| Height: | 205 mm |
| Depth: | 20 mm |
| Width with packaging: | 227 mm |
| Height with packaging: | 208 mm |
| Depth with packaging: | 78 mm |
| Range: | K |
| GTIN (EAN): | 4012799101376 |
| Article number: | E192.0801.0000 |

Manufacturer: MAICO

DI WS 75 Sealing