**Air filter, replacement Duo M6**

Replacement air filter for decentralised ventilation unit with Duo heat recovery.

Technical data

|  |  |
| --- | --- |
| Article: | Duo M6 |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material |
| Colour: | Black / white |
| Weight: | 0,04 kg |
| Weight including packaging: | 0,04 kg |
| Filter class: | ISO ePM2,5 ≥ 50 % (M6) |
| Width: | 210 mm |
| Height: | 113 mm |
| Depth: | 33 mm |
| Width with packaging: | 211 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 34 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799990970 |
| Article number: | 0093.1439 |

Manufacturer: MAICO

Duo M6 Air filter, replacement